# Финальный набор промптов · версия 3

Режим: встроенный ImageGen, генерация согласованных архитектурных визуализаций по исходным референсам.

## Общая спецификация проекта

```text
Create a premium photorealistic, structurally credible ROSATOM exhibition stand for a youth science and technology forum. The footprint is exactly 28 m long by 10 m deep, an elongated 2.8:1 composition with a clear 2.2 m public promenade along the open front.

Preserve the complete functional layout and every exhibit from the supplied rough 3D references. Equipment and interactive technology displays remain on the left, the central zone contains a separate transparent media art object plus negotiation tables, and the right zone is an open 36-person lecture theater. Do not delete, merge, replace, miniaturize or hide any exhibit as furniture. If an exhibit is occluded by the chosen camera, it must still remain physically present in the same stand. Inventory changes require explicit approval.

Concept: “Energy Contour”. A satin-white architectural base unifies portals, plinths, canopies and the lecture theater. It is not the art object. The primary art object is a freestanding multilayer transparent cubic “energy aquarium” positioned at the front center of the stand, visually separate from the negotiation furniture and from the upper ring.

CENTRAL ART OBJECT — mandatory visual invariant:
- one distinct transparent cubic volume, approximately 4.5–5.0 m wide, 4.0–4.5 m deep and 3.8–4.2 m high;
- five to seven visibly separated layers of clear low-iron glass, optical acrylic, dichroic glass and partial mirror surfaces;
- protected holographic LED fan displays positioned behind the transparent layers, producing floating scientific projections with real optical depth;
- layered reflections of projections, people and colored zones, with controlled dichroic cyan, magenta and violet shifts;
- a discreet technical plinth containing structure, cables, controllers and ventilation;
- transparent, visually permeable and scientifically intriguing, not a closed room, not a single glass showcase, not a generic LED cube;
- no seats, meeting tables or solid walls inside the art object;
- rotating projection hardware remains safely inaccessible behind certified transparent protection.

UPPER RING — separate architectural element:
The large upper ring is a canopy and branding crown only. Keep a clear air gap between the crown and the transparent cube so that they cannot be mistaken for one object. The crown may carry one approved ROSATOM fascia or remain blank. It must never replace, absorb or become the central art object.

LEFT EQUIPMENT ZONE:
Retain the full assortment and count of all source-reference exhibits, including every large, small, tall, cylindrical, tabletop and floor-standing unit, the transparent protected exhibit, media portal, interactive screens and demonstrator position. Use individual credible plinths and at least 1.4–1.5 m circulation where required. Give the zone a cyan/turquoise identity through light, graphics and selected surfaces while preserving the real forms of the equipment.

CENTRAL NEGOTIATION ZONE:
Place the complete negotiation program beside and behind the art object, never inside it. Use separate lightweight tables, comfortable seating and small acoustic elements. Color-code the zone with coral, magenta and warm pink accents. Preserve accessible clearances and keep all transparent layers of the art object visible from the public promenade.

RIGHT LECTURE THEATER:
Create an open 36-person amphitheater with four or five shallow rows, accessible positions integrated into the first row, a central aisle, two visible exits, low accessible stage and one large 16:9 media wall. Use indigo, violet and deep blue-violet acoustic surfaces with controlled stage lighting.

MATERIAL AND COLOR SYSTEM:
White and ice-gray solid-surface architecture forms the neutral structural base. Use purposeful, clearly legible color zoning: cyan/turquoise for equipment, coral/magenta for negotiation, indigo/violet for lecture, and transparent/dichroic/reflective materials for the art object. Add brushed aluminum, pale oak and tactile textiles. The result should be energetic, young and scientific, not sterile and not a random rainbow.

LIGHTING:
Professional neutral 4000 K exhibition illumination; museum-grade accents on every exhibit; cyan/turquoise tech-zone light; flattering coral/magenta negotiation light; separately controlled indigo/violet lecture lighting. The art object uses synchronized transparent projections, reflections and restrained dichroic glow. No strobing, exposed fan blades or nightclub lighting.

Populate the stand with a moderate number of diverse young adult visitors naturally using every zone. Maintain realistic human scale, anatomy, materials, safety detailing, construction joints, sightlines and circulation.

BRANDING:
Reserve one clean fascia on the upper architectural crown for the approved official mark. Render only one exact wordmark “РОСАТОМ”, or leave it blank. No other readable text.

Avoid: missing central art object; treating the upper ring as the art object; invented opaque central architecture; removing exhibits; reducing the equipment zone to a few generic plinths; negotiation furniture inside the cube; closed opaque cube; one flat screen pretending to be a multilayer installation; exposed spinning blades; sterile all-white interior; random rainbow blocks; neon green or yellow cubes; radiation signs; literal reactor imagery; spaceship interior; cheap glossy plastic; blocked aisles; inaccessible seating; fisheye distortion; fake Cyrillic; random logos; webpage UI; watermark.
```

## Ракурс 1 — главный широкий вид

```text
Use the shared version 3 specification. Camera at the open front-left corner, elevated about 3.5 m, 24 mm architectural lens, straight verticals. Show the complete 28 m stand in one panoramic frame. The freestanding transparent cubic “energy aquarium” must be prominent in the front center, with five to seven optical layers, floating holographic fan projections and reflections clearly readable. Show the full equipment-rich cyan/turquoise zone on the left, coral/magenta negotiation zone around and behind the cube, and active indigo/violet lecture theater on the right. Keep the upper white ring visually detached as the architectural branding crown. Neutral dark exhibition-hall background; high-end competition presentation render.
```

## Ракурс 2 — аксонометрия

```text
Use the shared version 3 specification and preserve the exact same stand and complete exhibit inventory. High front-left bird’s-eye camera, 55–60 degrees downward, near-orthographic architectural perspective. Show the entire 28 x 10 m footprint with generous margin. Make every equipment footprint, clear front promenade, transverse aisle, freestanding front-center art cube, separate negotiation furniture, amphitheater rows, accessible positions and two lecture exits easy to read. Show the five to seven transparent layers inside the cube and the air gap below the separate upper branding crown. Clean light-neutral presentation background; reduced crowd.
```

## Ракурс 3 — вид посетителя

```text
Use the shared version 3 specification and preserve the exact same stand and complete exhibit inventory. Eye height 1.65 m, 24–28 mm architectural lens, camera on the clear front promenade slightly left of center, looking diagonally through the transparent front-center “energy aquarium” toward the lecture theater. Make the layered glass, acrylic, dichroic reflections and protected holographic LED fan projections the hero of the image. Keep a substantial portion of the cyan/turquoise equipment zone visible at the left edge, coral/magenta negotiation activity beside the cube, and the indigo/violet lecture theater active on the right. The upper ring remains a clearly separate canopy and branding crown. Wide cinematic 16:9 composition, realistic, energetic and welcoming.
```
